Clean up all parts.

A picture containing text, blue, bin, container

Description automatically generated

Put 2mm nut in hole for coupling.

A picture containing grass, green


Description automatically generated

Use 2mm x 10 bolt and screw into nut, make sure it swivels freely then put drop of superglue onto nut and end of bolt.

A picture containing grass

Description automatically generated

Glue 2 x 2mm nuts into chassis at front of tender.



Bolt chassis to tender body with 2 x 2mm x 6mm bolts at front and 2 x 2mm x 8mm bolts at near, with nuts underside.

A picture containing green, blue

Description automatically generated

Put 5 x 2mm nuts either side into slots in chassis. Glue 1/8 brass bearings into metal side frames from the inside ( you may have to file the holes out ).

Bolt 1 side frame with 2 x 10mm bolts into captive nuts. Put wheels onto axles ( 28mm inside flange ). Put axles into bearings and bolt the other side frame on.

A picture containing text, blue

Description automatically generated

Glue axles boxes to side frames.

A picture containing text, blue

Description automatically generated

Complete Tender

A picture containing indoor, green, case, accessory

Description automatically generated